ADL(4) | Device Drivers Manual | ADL(4)

# NAME

`adl` — Andigilog aSC7621 temperature, voltage, and fan sensor

# SYNOPSIS

`adl* at iic?`

# DESCRIPTION

The `adl` driver provides support for the Andigilog aSC7621 sensors. The sensor possesses a collection of sensor values which are made available through the sysctl(8) interface.

# SEE ALSO

iic(4), intro(4), sensorsd(8), sysctl(8)

# HISTORY

The `adl` driver first appeared in OpenBSD 4.3.

# AUTHORS

The `adl` driver was written by Mike Belopuhov.

July 12, 2012 | Debian