ACX(4) | Device Drivers Manual | ACX(4)

# NAME

`acx` — TI ACX100/ACX111 IEEE 802.11a/b/g wireless network device

# SYNOPSIS

`acx* at cardbus?`
`acx* at pci?`

# DESCRIPTION

The `acx` driver provides support for TI TNETW1100/TNETW1100B (ACX100) and TNETW1130 (ACX111) based PCI/CardBus network adapters.

The ACX100A and ACX100B are first generation 802.11b devices from TI. The ACX111 is a second generation device which supports 802.11b/g and in some cases 802.11a.

These are the modes the `acx` driver can operate in:

BSS mode
  Also known as infrastructure mode, this is used when associating with an access point, through which all traffic passes. This mode is the default.
IBSS mode
  Also known as IEEE ad-hoc mode or peer-to-peer mode. This is the standardized method of operating without an access point. Stations associate with a service set. However, actual connections between stations are peer-to-peer.
Host AP
  In this mode the driver acts as an access point (base station) for other cards.
monitor mode
  In this mode the driver is able to receive packets without associating with an access point. This disables the internal receive filter and enables the card to capture packets from networks which it wouldn't normally have access to, or to scan for access points.

The `acx` driver can be configured to use Wired Equivalent Privacy (WEP) in software for ACX111 or in hardware for ACX100. It is strongly recommended that WEP not be used as the sole mechanism to secure wireless communication, due to serious weaknesses in it.

The transmit speed is user-selectable or can be adapted automatically by the driver depending on the number of hardware transmission retries.

In Host AP mode, the driver is compatible with clients using powersave.

The `acx` driver can be configured at runtime with ifconfig(8) or on boot with hostname.if(5).

# FILES

The driver needs a set of firmware files which are loaded when an interface is brought up:

/etc/firmware/tiacx100
/etc/firmware/tiacx100r0D
/etc/firmware/tiacx100r11
/etc/firmware/tiacx111
/etc/firmware/tiacx111c16
/etc/firmware/tiacx111r16

These firmware files are not free because TI refuses to grant distribution rights. In fact they have rebuffed thousands of attempts to start a dialogue on this issue. As a result, even though OpenBSD includes the driver, the firmware files cannot be included and users have to download these files on their own.

A prepackaged version of the firmware can be installed using fw_update(8).

# HARDWARE

The following cards are among those supported by the `acx` driver:

Card | Chip | Bus | Standard
D-Link DWL-520+ | ACX100 | PCI | b
D-Link DWL-650+ | ACX100 | CardBus | b
D-Link DWL-G520+ | ACX111 | PCI | b/g
D-Link DWL-G630+ | ACX111 | CardBus | b/g
D-Link DWL-G650+ | ACX111 | CardBus | b/g
Digitus DN-7001G | ACX111 | CardBus | b/g
Ergenic ERG WL-003 | ACX100 | CardBus | b
Hamlet HNWP254 | ACX111 | CardBus | b/g
Hawking HWP54G | ACX111 | PCI | b/g
Linksys WPC54Gv2 | ACX111 | CardBus | b/g
Microcom Travelcard | ACX111 | CardBus | b/g
Netgear WG311v2 | ACX111 | PCI | b/g
Sceptre SC254W+ | ACX111 | CardBus | b/g
Tornado/ADT 211g | ACX111 | PCI | b/g
USR USR5410 | ACX111 | CardBus | b/g
USR USR5416 | ACX111 | PCI | b/g
ZyXEL G-160 | ACX111 | CardBus | b/g
ZyXEL G-360 EE | ACX111 | PCI | b/g

# EXAMPLES

The following example scans for available networks:

`# ifconfig acx0 scan`

The following hostname.if(5) example configures acx0 to join network “mynwid”, using WEP key “mywepkey”, obtaining an IP address using DHCP:

    nwid mynwid nwkey mywepkey
    inet autoconf

The following hostname.if(5) example creates a host-based access point on boot:

    mediaopt hostap
    nwid mynwid nwkey mywepkey
    inet 192.168.1.1 255.255.255.0

# SEE ALSO

arp(4), cardbus(4), ifmedia(4), intro(4), netintro(4), pci(4), hostname.if(5), hostapd(8), ifconfig(8)

# HISTORY

The `acx` driver first appeared in OpenBSD 4.0.

# AUTHORS

The `acx` driver was written by Sepherosa Ziehau. The manual page was written by Sascha Wildner. Both are based on the http://wlan.kewl.org project team's original code.

The hardware specification was reverse engineered by the good folks at http://acx100.sourceforge.net. Without them this driver would not have been possible.

January 5, 2022 | Debian