SXIE(4) | Device Drivers Manual (armv7) | SXIE(4)

# NAME

`sxie` — A1X/A20 EMAC 10/100 Ethernet device

# SYNOPSIS

`sxie* at fdt?`

# DESCRIPTION

The `sxie` driver provides support for the EMAC 10/100 Ethernet device integrated in Allwinner Technology A1X/A20 SoCs. For more information on configuring this device, see ifconfig(8).

# SEE ALSO

ifmedia(4), mii(4), hostname.if(5), ifconfig(8)

# HISTORY

The `sxie` device driver first appeared in OpenBSD 5.5.

June 26, 2016 | Debian