QLW(4) | Device Drivers Manual | QLW(4)

# NAME

`qlw` — QLogic ISP1000/1020/1x40/1x80/1x160 SCSI controller

# SYNOPSIS

`qlw* at pci?`
`qlw* at sbus?`

# DESCRIPTION

The `qlw` driver provides support for QLogic Ultra Wide SCSI host bus adapters using the ISP1000, ISP1020/1040, ISP1080/1240/1280 and ISP10160/12160 chips.

`qlw` provides no ability to configure an adapter's parameters at runtime; all configuration must be done prior to booting OpenBSD.

# SEE ALSO

intro(4), pci(4), qla(4), qle(4), sbus(4), scsi(4)

# HISTORY

The `qlw` driver first appeared in OpenBSD 5.6.

# AUTHORS

The `qlw` driver was written by Mark Kettenis <kettenis@openbsd.org>, based on the qla(4) driver written by Jonathan Matthew <jmatthew@openbsd.org>.

January 21, 2015 | Debian