GPIOKEYS(4) | Device Drivers Manual | GPIOKEYS(4)

# NAME

`gpiokeys` — GPIO keys

# SYNOPSIS

`gpiokeys* at fdt?`

# DESCRIPTION

The `gpiokeys` driver handles events triggered by GPIO keys. Currently, only lid status events are supported.

The lid status is set up as a sensor and can be monitored using sysctl(8) or sensorsd(8).

# SEE ALSO

gpio(4), intro(4), sensorsd(8), sysctl(8)

# HISTORY

The `gpiokeys` driver first appeared in OpenBSD 7.1.

# AUTHORS

The `gpiokeys` driver was written by Klemens Nanni <kn@openbsd.org>.

November 9, 2021 | Debian