GPIOIIC(4) | Device Drivers Manual | GPIOIIC(4)

# NAME

`gpioiic` — GPIO I2C controller

# SYNOPSIS

`gpioiic* at gpio? offset 0 mask 0x3 flag 0x0`
`gpioiic* at gpio?`
`iic* at gpioiic?`

# DESCRIPTION

The `gpioiic` driver allows bit-banging an I2C bus as a master using two GPIO pins. By default the first pin is used as a serial data (SDA) signal and the second as a serial clock (SCL). If the flag locator is set to 0x01, the order of the SDA and SCL signals is reversed. Both GPIO pins must be able to drive an output and the SDA pin must be also able to read an input.

The pins can be specified in the kernel configuration with the offset and the mask locators. The offset and mask can also be specified when `gpioiic` is attached at runtime using the `GPIOATTACH` ioctl(2) on the gpio(4) device. Each bit in the mask locator defines one pin; the pin number is calculated as an addition of the bit position and the offset locator. For example, offset 17 and mask 0x5 defines pin numbers 17 and 19.

# SEE ALSO

gpio(4), iic(4), intro(4)

# HISTORY

The `gpioiic` driver first appeared in OpenBSD 3.9.

# AUTHORS

The `gpioiic` driver was written by Alexander Yurchenko <grange@openbsd.org>.

July 16, 2013 | Debian