RKCOMPHY(4) | Device Drivers Manual | RKCOMPHY(4)

# NAME

`rkcomphy` — Rockchip PCIe/USB3/SATA/QSGMII PHY

# SYNOPSIS

`rkcomphy* at fdt?`

# DESCRIPTION

The `rkcomphy` driver controls the combo PIPE PHY integrated on Rockchip RK3566/RK3568 and RK3588 SoCs. The PHY supports the PCIe 2.0 (2.5 GT/s and 5 GT/s), USB 3.0 (5 Gbps), SATA (1.5 Gbit/s, 3 Gbit/s and 6 Gbit/s) and QSGMII (1.25 Gbit/s and 5 Gbit/s) protocols. The `rkcomphy` driver does not implement support for QSGMII.

# SEE ALSO

intro(4)

# HISTORY

The `rkcomphy` device driver first appeared in OpenBSD 7.3.

# AUTHORS

The `rkcomphy` driver was written by Mark Kettenis <kettenis@openbsd.org>.

March 12, 2023 | Debian