BCMAUX(4) | Device Drivers Manual | BCMAUX(4)

# NAME

`bcmaux` — Broadcom BCM283x auxiliary peripherals

# SYNOPSIS

`bcmaux* at fdt?`

# DESCRIPTION

The `bcmaux` driver handles clock gating and interrupts for the auxiliary peripherals in the Broadcom BCM2835, BCM2836 and BCM2837 SoCs.

# SEE ALSO

intro(4)

# HISTORY

The `bcmaux` driver first appeared in OpenBSD 6.2.

# AUTHORS

The `bcmaux` driver was written by Mark Kettenis <kettenis@openbsd.org>.

April 1, 2018 | Debian