LE(4) | Device Drivers Manual (i386) | LE(4)

# NAME

`le` — AMD LANCE Ethernet device

# SYNOPSIS

`le0 at isa? port 0x360 irq 15 drq 6`
`le* at isapnp?`

# DESCRIPTION

The `le` interface provides access to a 10 Mb/s Ethernet network via the AMD LANCE Ethernet chips. This includes the following models:

AT&T StarLAN 10, EN100, and StarLAN Fiber
BICC Isolan
BOCALANcard
Digital DEPCA
Kingston 21xx
Novell NE1500T
Novell NE2100

# SEE ALSO

arp(4), ifmedia(4), intro(4), isa(4), isapnp(4), netintro(4), hostname.if(5), ifconfig(8)

May 31, 2007 | Debian