MAXDS(4) | Device Drivers Manual | MAXDS(4)

# NAME

`maxds` — Maxim DS1624/DS1631/DS1721 temperature sensor

# SYNOPSIS

`maxds* at iic?`

# DESCRIPTION

The `maxds` driver provides support for the Maxim DS1624/DS1631/DS1721 temperature sensor. The sensor possesses just one accurate temperature sensor; the value is made available through the sysctl(8) interface.

# SEE ALSO

iic(4), intro(4), sensorsd(8), sysctl(8)

# HISTORY

The `maxds` driver first appeared in OpenBSD 3.9.

# AUTHORS

The `maxds` driver was written by Theo de Raadt <deraadt@openbsd.org>.

July 16, 2013 | Debian