WBENV(4) | Device Drivers Manual | WBENV(4)

# NAME

`wbenv` — Winbond W83L784R/W83L785R/W83L785TS-L temperature, voltage, and fan sensor

# SYNOPSIS

`wbenv* at iic?`

# DESCRIPTION

The `wbenv` driver provides support for the Winbond W83L784R, W83L785R and W83L785TS-L hardware monitors to be used with the sysctl(8) interface.

The W83L874R and W83L785R possess several voltage, temperature and fan speed sensors. The W83L785TS-L only has a single temperature sensor.

# SEE ALSO

iic(4), intro(4), sensorsd(8), sysctl(8)

# HISTORY

The `wbenv` driver first appeared in OpenBSD 3.9.

# AUTHORS

The `wbenv` driver was written by Mark Kettenis <kettenis@openbsd.org>.

July 16, 2013 | Debian