AMLPINCTRL(4) | Device Drivers Manual | AMLPINCTRL(4)

# NAME

`amlpinctrl` — Amlogic pin multiplexing

# SYNOPSIS

`amlpinctrl* at fdt?`

# DESCRIPTION

The `amlpinctrl` driver uses pin control data from the device tree to select one of multiple possible roles available for pins on Amlogic SoCs.

# SEE ALSO

intro(4)

# HISTORY

The `amlpinctrl` device driver first appeared in OpenBSD 6.6.

# AUTHORS

The `amlpinctrl` driver was written by Mark Kettenis <kettenis@openbsd.org>.

August 28, 2019 | Debian