PINCTRL(4) | Device Drivers Manual | PINCTRL(4)

# NAME

`pinctrl` — generic pin multiplexing

# SYNOPSIS

`pinctrl* at fdt?`

# DESCRIPTION

The `pinctrl` driver uses pin control data from the device tree to select one of multiple possible roles available for pins on various SoCs.

# SEE ALSO

intro(4)

# HISTORY

The `pinctrl` device driver first appeared in OpenBSD 6.4.

# AUTHORS

The `pinctrl` driver was written by Mark Kettenis <kettenis@openbsd.org>.

August 26, 2018 | Debian