ANDL(4) | Device Drivers Manual | ANDL(4)

# NAME

`andl` — Andigilog aSC7611 temperature, voltage, and fan sensor

# SYNOPSIS

`andl* at iic?`

# DESCRIPTION

The `andl` driver provides support for the Andigilog aSC7611 hardware monitor. The device provides 3 temperature sensors, 5 voltage sensors and 4 fan sensors. Sensor values are made available through the sysctl(8) interface.

# SEE ALSO

iic(4), intro(4), sensorsd(8), sysctl(8)

Andigilog aSC7611 Hardware Monitor with Integrated Fan Control, October 2006.

# HISTORY

The `andl` driver first appeared in OpenBSD 4.4.

# AUTHORS

The `andl` driver was written by Constantine A. Murenin <cnst@openbsd.org> whilst at the University of Waterloo.

February 18, 2022 | Debian