WDS(4) | Device Drivers Manual (i386) | WDS(4)

# NAME

`wds` — WD7000 compatible ISA SCSI interface

# SYNOPSIS

`wds0 at isa? port 0x350 irq 15 drq 6 # WD7000, TMC-7000`
`wds1 at isa? port 0x358 irq 11 drq 5`

# DESCRIPTION

The `wds` driver supports the WD7000 family of SCSI adapters and compatibles, including:

WD7000-ASC
  Busmastering DMA controller.
WD7000-ASE
  An ASC with floppy controller and ESDI, manufactured for Apollo workstations.
WD7000-FASST2
  An ASC with new firmware and scatter-gather hardware.

# SEE ALSO

cd(4), ch(4), intro(4), isa(4), scsi(4), sd(4), st(4)

August 14, 2012 | Debian