BMTPHY(4) | Device Drivers Manual | BMTPHY(4)

# NAME

`bmtphy` — Broadcom Mini-Theta Ethernet PHY

# SYNOPSIS

`bmtphy* at mii?`

# DESCRIPTION

The `bmtphy` driver supports the Broadcom Mini-Theta BCM5201 and BCM5202 10/100 Ethernet PHYs and their derivatives such as BCM4401, BCM5214, and BCM522x. It also supports the internal PHY on the 3Com 3C905C-TX 10/100 Ethernet interface, and the internal PHY on some 3Com 3C905B-TX 10/100 Ethernet interfaces. These PHYs are found on a variety of Ethernet interfaces.

# SEE ALSO

ifmedia(4), intro(4), mii(4), ifconfig(8)

January 24, 2020 | Debian