LII(4) | Device Drivers Manual | LII(4)

# NAME

`lii` — Attansic L2 10/100 Ethernet device

# SYNOPSIS

`lii* at pci?`
`atphy* at mii?`

# DESCRIPTION

The `lii` driver provides support for Ethernet interfaces based on the Attansic L2 Ethernet chipset.

The `lii` driver supports the following media types:

`autoselect`
  Enable autoselection of the media type and options. The user can manually override the autoselected mode by adding media options to the appropriate hostname.if(5) file.
`10baseT`
  Set 10Mbps operation. The ifconfig(8) `mediaopt` option can also be used to select either `full-duplex` or `half-duplex` modes.
`100baseTX`
  Set 100Mbps (Fast Ethernet) operation. The ifconfig(8) `mediaopt` option can also be used to select either `full-duplex` or `half-duplex` modes.

The `lii` driver supports the following media options:

`full-duplex`
  Force full duplex operation.
`half-duplex`
  Force half duplex operation.

For more information on configuring this device, see ifconfig(8). To view a list of media types and options supported by the card, try `ifconfig <device> media`. For example, `ifconfig lii0 media`.

# SEE ALSO

arp(4), atphy(4), ifmedia(4), intro(4), netintro(4), pci(4), hostname.if(5), ifconfig(8)

# HISTORY

The `lii` device driver first appeared in OpenBSD 4.3.

# AUTHORS

The `lii` driver was written by Quentin Garnier.

January 27, 2011 | Debian