IO(4) | Device Drivers Manual (hppa) | IO(4)

# NAME

`io` — HP PA-RISC I/O subsystem reference

# DESCRIPTION

The following table lists the PA-RISC I/O subsystems and connected devices found in the supported HP 9000/700 machines.

Model | MBA | SCSI | Network | Video | Misc
705 | A | SE | DX | Timber |
710 | A | SE | DX | Timber |
712 | LW | SE | CA, TR | Artist |
715/33 | A | SE | DX | Stinger |
715/50 | A | SE | DX | Stinger |
715/64 | LW | SE | CA | Artist |
715/75 | A | SE | DX | Stinger |
715/80 | LW | SE | CA | Artist |
715/100 | LW | SE | CA | Artist |
720 | A | SE | DX | [SGC] |
725/50 | A | SE | DX | Stinger |
725/75 | A | SE | DX | Stinger |
725/64 | LW | SE | CA | Artist |
725/100 | LW | SE | CA | Artist |
730 | A | SE | DX | [SGC] |
735 | A | SE, FWD | DX, FDDI | [SGC] |
742i | A | SE | CA | Stinger | VME
743i | DLW | SE | DX | Artist | VME
744 | DLW | SE | DX | EG | VME
745 | DLW | SE | DX | EG | VME
745i | A | SE | DX | Stinger |
747i | A | SE | DX | Stinger |
748 | DLW | SE | DX | EG | VME
748i | DLW | SE | DX | Artist | VME
750 | A | SE | DX | [SGC] |
755 | A | SE, FWD | DX, FDDI | [SGC] |
A180/C | DL | SE | DC | [GSC/PCI] |
B132L | DLW | SE, FWD | CA | EG |
B160L | DLW | SE, UW | DC | EG |
B180L | DLW | SE, UW | DC | EG |
C100 | LUW | SE, FWD | CA | [GSC] |
C110 | LUW | SE, FWD | CA | [GSC] |
C132L | DLUW | SE, UW | DC | EG |
C160L | DLUW | SE, UW | DC | EG |
C160 | DLU | SE, UW | DC | [GSC/PCI] |
C180L | DLUW | SE, UW | DC | EG |
C180 | DLU | SE, UW | DC | [GSC/PCI] |
C200 | DLU | SE, UW | DC | [GSC/PCI] |
C230 | DLU | SE, UW | DC | [GSC/PCI] |
C240 | DLU | SE, UW | DC | [GSC/PCI] |
C360 | DLU | SE, UW | DC | [GSC/PCI] |
J200 | LUW | SE, FWD | CA | [GSC] |
J210/XC | LUW | SE, FWD | CA | [GSC] |
J280 | DLUW | SE, UW | DC | [GSC/PCI] |
J282 | DLUW | SE, UW | DC | [GSC/PCI] |
J2240 | DLUW | SE, UW | DC | [GSC/PCI] |
RDI | DL | SE | CA | EG | CardBus
SAIC | LW | SE | CA | Artist | PCMCIA

The MBA column denotes the bus adapters in use:

A
  asp(4)
D
  dino(4)
L
  lasi(4)
U
  uturn(4)
W
  wax(4)

The trailing characters in the SCSI row denote the SCSI bus configuration:

SE
  oosiop(4) or osiop(4); Symbios/NCR 53C700/710 8-bit (fast) single-ended,
FWD
  siop(4); NCR53C720 16-bit fast differential (HVD),
UW
  siop(4); NCR53C875 16-bit ultra single-ended.

The trailing digits in the Network row denote the interface speed:

CA
  ie(4); i82596CA 10 Mb/s,
DX
  ie(4); i82596DX 10 Mb/s,
DC
  dc(4); DEC 21142/3 10/100 Mb/s,
FDDI
  Am78830 Formac+ FDDI.

# SEE ALSO

asp(4), dc(4), dino(4), gsc(4), ie(4), intro(4), lasi(4), oosiop(4), osiop(4), runway(4), siop(4), sti(4), uturn(4), wax(4)

# HISTORY

The hppa `io` reference first appeared with OpenBSD 3.3.

September 3, 2011 | Debian