AGE(4) | Device Drivers Manual | AGE(4)

# NAME

`age` — Attansic L1 10/100/1Gb Ethernet device

# SYNOPSIS

`age* at pci?`
`atphy* at mii?`

# DESCRIPTION

The `age` driver provides support for Ethernet interfaces based on the Attansic L1 Ethernet chipset.

The `age` driver supports IPv4 receive IP/TCP/UDP checksum offload and VLAN tag insertion and stripping.

The following media types are supported:

`autoselect`
  Enable autoselection of the media type and options.
`10baseT`
  Set 10Mbps operation.
`100baseTX`
  Set 100Mbps (Fast Ethernet) operation.
`1000baseT`
  Set 1000Mbps (Gigabit Ethernet) operation.

For more information on configuring this device, see ifconfig(8). To view a list of media types and options supported by the card, try `ifconfig <device> media`. For example, `ifconfig age0 media`.

# SEE ALSO

arp(4), atphy(4), ifmedia(4), intro(4), netintro(4), pci(4), hostname.if(5), ifconfig(8)

# HISTORY

The `age` device driver first appeared in OpenBSD 4.5.

# AUTHORS

The `age` driver was written by Pyun YongHyeon for FreeBSD and ported to OpenBSD by Kevin Lo <kevlo@openbsd.org>.

September 8, 2021 | Debian