DWQE(4) | Device Drivers Manual | DWQE(4)

# NAME

`dwqe` — Synopsys DesignWare Ethernet Quality-of-Service Controller

# SYNOPSIS

`dwqe* at fdt?`
`dwqe* at pci?`

# DESCRIPTION

The `dwqe` driver provides support for various Ethernet controllers based on the Synopsys DesignWare Ethernet Quality-of-Service Controller IP. These controllers are found on Rockchip RK3566, RK3568, and RK3588 SoCs, and on Intel Elkhart Lake SoCs.

The `dwqe` driver supports several media types, which are selected via the ifconfig(8) command. The supported media types are:

`media` autoselect
  Attempt to autoselect the media type (default)
`media` 1000baseT `mediaopt` full-duplex
  Use 1000baseT on copper, full duplex
`media` 1000baseT `mediaopt` half-duplex
  Use 1000baseT on copper, half duplex
`media` 100baseTX `mediaopt` full-duplex
  Use 100baseTX, full duplex
`media` 100baseTX `mediaopt` half-duplex
  Use 100baseTX, half duplex

# SEE ALSO

arp(4), ifmedia(4), inet(4), intro(4), netintro(4), hostname.if(5), ifconfig(8)

# HISTORY

OpenBSD support for `dwqe` first appeared in OpenBSD 7.3.

October 11, 2023 | Debian