MFI(4) | Device Drivers Manual | MFI(4)

# NAME

`mfi` — LSI Logic & Dell MegaRAID SAS RAID controller

# SYNOPSIS

`mfi* at pci?`

# DESCRIPTION

The `mfi` driver provides support for the MegaRAID SAS family of RAID controllers, including:

- Dell PERC 5/e, PERC 5/i, PERC 6/e, PERC 6/i, PERC H310, PERC H700, PERC H800
- IBM ServeRAID M1115
- Intel RAID Controller SRCSAS18E, SRCSAS144E
- LSI Logic MegaRAID SAS 8300XLP, MegaRAID SAS 8308ELP, MegaRAID SAS 8344ELP, MegaRAID SAS 8408E, MegaRAID SAS 8480E, MegaRAID SAS 8880EM2, MegaRAID SAS 8888ELP, MegaRAID SAS 9240-4i, MegaRAID SAS 9240-8i, MegaRAID SAS 9260-16i, MegaRAID SAS 9260-4i, MegaRAID SAS 9260-8i, MegaRAID SAS 9260CV-4i, MegaRAID SAS 9260CV-8i, MegaRAID SAS 9261-8i, MegaRAID SAS 9265-8i, MegaRAID SAS 9280-16i4e, MegaRAID SAS 9280-24i4e, MegaRAID SAS 9280-4i4e, MegaRAID SAS 9280-8e, MegaRAID SAS 9285-8e

These controllers support RAID 0, RAID 1, RAID 5, RAID 6, RAID 10, RAID 50 and RAID 60 using either SAS or SATA II drives.

Although the controllers are actual RAID controllers, the driver makes them look just like SCSI controllers. All RAID configuration is done through the controllers' BIOSes.

# SEE ALSO

bio(4), intro(4), pci(4), scsi(4), sd(4), bioctl(8), sensorsd(8), sysctl(8)

# HISTORY

The `mfi` driver first appeared in OpenBSD 4.0.

# AUTHORS

The `mfi` driver was written by Marco Peereboom <marco@openbsd.org>.

November 8, 2013 | Debian