EAP(4) | Device Drivers Manual | EAP(4)

# NAME

`eap` — Ensoniq AudioPCI audio device

# SYNOPSIS

`eap* at pci?`
`audio* at eap?`
`midi* at eap?`

# DESCRIPTION

The `eap` driver supports the older Ensoniq AudioPCI and other ES1370 based sound cards, such as the Creative Labs SoundBlaster PCI64 and PCI128. The driver also supports many revisions of the more modern Ensoniq AudioPCI 97 (ES1371), as well as the Ensoniq CT5880 and the Creative Labs Ectiva 1938.

# SEE ALSO

ac97(4), audio(4), intro(4), midi(4), pci(4)

# HISTORY

The `eap` device driver appeared in OpenBSD 2.6.

# BUGS

The "FM" DAC is not supported.

June 26, 2008 | Debian