DWCTWO(4) | Device Drivers Manual | DWCTWO(4)

# NAME

`dwctwo` — DesignWare HS USB 2.0 OTG controller

# SYNOPSIS

`dwctwo* at fdt?` (arm64, armv7)
`dwctwo0 at iobus? irq 56` (octeon)
`usb* at dwctwo?`

# DESCRIPTION

The `dwctwo` driver provides support for the DesignWare High-Speed USB 2.0 On-the-Go controller, which provides an interface to usb(4) devices.

# SEE ALSO

ehci(4), ohci(4), usb(4), xhci(4)

# HISTORY

The `dwctwo` driver first appeared in OpenBSD 5.8.

February 17, 2017 | Debian