MSTS(4) | Device Drivers Manual | MSTS(4)

# NAME

`msts` — Meinberg Standard Time String timedelta sensor

# SYNOPSIS

`pseudo-device msts` [count]

# DESCRIPTION

This line discipline interfaces serial Meinberg devices.

The line discipline is enabled by the following sequence:

    #include <sys/ioctl.h>
    int ldisc = MSTSDISC, fildes; ...
    ioctl(fildes, TIOCSETD, &ldisc);

The byte stream is unaltered by the line discipline which maintains a timedelta sensor using the MSTS data. The timedelta sensor will appear as msts* in the list of sensors and the delta (in nanoseconds) between the received time information and the local time can be accessed through the sysctl(8) interface.

The Meinberg radio clocks use the following default baudrates:

GPS-receivers (external and PCI, COM0)
  19200/8N1
GPS-receivers (external, COM1)
  9600/8N1
DCF77-receivers (external)
  9600/7E2
DCF77-receivers (PCI)
  4800/8N1

# SENSOR STATES

The quality of the timedelta is reported as the sensor status:

OK
  The time information is valid. The timedelta is safe to use for applications like ntpd(8).
WARN
  The attached receiver has been indicating a warning condition for at least the last ten minutes. The timedelta should be used with care.
CRITICAL
  tty timestamping has been turned on but there is no PPS signal present or the receiver indicated a warning condition for at least the last twenty minutes. Check your hardware. Some receiver units need PPS to be manually turned on.

The status of a second sensor is used to report the status of the device itself:

OK
  The clock is synchronized, e.g. a GPS receiver has a fix.
WARN
  The device issued a warning condition, e.g. a GPS receiver has no fix.

# SEE ALSO

tty(4), ldattach(8), ntpd(8), sysctl(8)

# HISTORY

The `msts` interface first appeared in OpenBSD 4.3.

# AUTHORS

The `msts` line discipline was written by Marc Balmer <mbalmer@openbsd.org>.

January 15, 2015 | Debian