UPLCOM(4) | Device Drivers Manual | UPLCOM(4)

# NAME

`uplcom` — Prolific PL-2303 USB serial adapter

# SYNOPSIS

`uplcom* at uhub?`
`ucom* at uplcom?`

# DESCRIPTION

The `uplcom` driver provides support for the Prolific PL-2303 USB-to-RS232 Bridge chip.

The device is accessed through the ucom(4) driver which makes it behave like a tty(4).

# HARDWARE

The `uplcom` driver supports the following adapters:

Alcatel One Touch 535/735
Aten UC232A
Belkin F5U257
Digitus DA-70145
ELECOM UC-SGT
Ericsson DCU-10 & DCU-11, made by Susteen, Inc.
HAL Crossam2+USB
HIGH-EDGE HE800
I/O DATA USB-RSAQ
I/O DATA USB-RSAQ2
I/O DATA USB-RSAQ3
I/O DATA USB-RSAQ5
IOGEAR UC-232A
iTegno WM1080A
Leadtek 9531 GPS
Maxxtro UC-232A
Nokia CA-42
Ours Technology DKU-5 clone
Palm 700WX
Pharos USB GPS
PLANEX USB-RS232 URS-03
RATOC REX-USB60
Samsung I330 cradle
Siemens X65
Siemens X75
Siemens SX1
Sitecom USB-Serial CNA-104
SOURCENEXT KeikaiDenwa 8
Speed Dragon MS3303H
TDK USB-PDC Adapter UPA9664
TDK USB-PHS Adapter UHA6400
Tripp-Lite U209

# SEE ALSO

intro(4), tty(4), ucom(4), uhub(4), usb(4)

# HISTORY

The `uplcom` driver appeared in NetBSD 1.6. OpenBSD support was added in OpenBSD 3.0.

August 8, 2017 | Debian