UWACOM(4) | Device Drivers Manual | UWACOM(4)

# NAME

`uwacom` — Wacom USB tablets

# SYNOPSIS

`uwacom* at uhidev?`
`wsmouse* at uwacom? mux 0`

# DESCRIPTION

The `uwacom` driver provides basic support for Wacom USB tablets. Access to these devices is through the wscons(4) framework.

Absolute positioning of the mouse cursor can be done by hovering the pen above the tablet. Touching the tablet with the pen tip will emulate mouse button 0, while the two pen buttons will emulate button 1 and button 2.

The `uwacom` driver supports the following Wacom tablets:

Name | Model Number
`Intuos Draw` | CTL-490
`Intuos S` | CTL-4100
`One S` | CTL-472
`One M` | CTL-672

# SEE ALSO

uhidev(4), usb(4), wsmouse(4)

# HISTORY

The `uwacom` driver first appeared in OpenBSD 6.1.

# AUTHORS

The `uwacom` driver was written by Frank Groeneveld <frank@frankgroeneveld.nl>. Support for “S” models was written by Vladimir Meshcheriakov <vladimir.meshcheriakov@epita.fr>.

# CAVEATS

Advanced features such as pen tip pressure are not supported.

August 12, 2023 | Debian