LC(4) | Device Drivers Manual | LC(4)

# NAME

`lc` — DEC EtherWORKS III 10/100 Ethernet device

# SYNOPSIS

`lc0 at isa? port 0x200`
`lc1 at isa? port 0x280`

# DESCRIPTION

The `lc` device driver supports DEC EtherWORKS III Ethernet interfaces, which are based on the LEMAC Ethernet chip. This includes the DE203, DE204, and DE205.

# MEDIA SELECTION

The EtherWORKS III series supports various combinations of media, depending on model. Some models also support media autoselect. Media is selected with ifconfig(8)'s ‘media’ directive.

# SEE ALSO

arp(4), ifmedia(4), intro(4), isa(4), netintro(4), hostname.if(5), ifconfig(8)

# HISTORY

The `lc` driver first appeared in NetBSD 1.3, OpenBSD support was added in OpenBSD 3.0.

# AUTHORS

The `lc` driver was written by Matt Thomas <matt@netbsd.org> and ported to OpenBSD by Niklas Hallqvist <niklas@openbsd.org>

# BUGS

The `lc` does not currently support EISA LEMAC interfaces.

July 16, 2013 | Debian