DINO(4) | Device Drivers Manual (hppa) | DINO(4)

# NAME

`dino` — Dino and Cujo Host/PCI bridges

# SYNOPSIS

`dino* at phantomas?`
`dino* at uturn?`
`com1 at dino? irq 11`
`pci* at dino?`

# DESCRIPTION

This driver supports Dino and Cujo Host/PCI bridges found on the A, B, C and J-class workstations. Cujo is a 64 bit datapath version of Dino.

On some machines it may also provide an additional serial port through the com(4) driver, or PS/2 keyboard and mouse ports, though the latter are not yet supported.

# SEE ALSO

com(4), intro(4), pci(4), phantomas(4), uturn(4)

# HISTORY

The `dino` driver appeared in OpenBSD 3.5.

# BUGS

`dino` bridges of revision earlier than three may exhibit data corruption on DMA. This hardware bug does not affect `cujo` or card mode `dino` bridges. See HP Service Note Numbers A4190A-01 and A4191A-01 for more details. Systems affected are those shipped before Aug 20, 1997 and of models: B132L, B160L, C160, C180, C200, C240.

May 31, 2007 | Debian