RKPINCTRL(4) | Device Drivers Manual | RKPINCTRL(4)

# NAME

`rkpinctrl` — Rockchip pin multiplexing

# SYNOPSIS

`rkpinctrl* at fdt?`

# DESCRIPTION

The `rkpinctrl` driver uses pin control data from the device tree to select one of multiple possible roles available for pins on Rockchip SoCs.

# SEE ALSO

intro(4)

# HISTORY

The `rkpinctrl` device driver first appeared in OpenBSD 6.2.

# AUTHORS

The `rkpinctrl` driver was written by Mark Kettenis <kettenis@openbsd.org>.

March 31, 2018 | Debian