OCE(4) | Device Drivers Manual | OCE(4)

# NAME

`oce` — Emulex OneConnect 10Gb Ethernet device

# SYNOPSIS

`oce* at pci?`

# DESCRIPTION

The `oce` driver supports Emulex OneConnect 10Gb Ethernet adapters based on the BladeEngine 2, BladeEngine 3 and Lancer chipsets, including the following:

- Emulex OCe11102 (SPF+/10GbaseSR or 10GbaseT)
- Emulex OCe10102 (SPF+/10GbaseSR)
- HP NC550M Flex-10 (10GbaseKR)
- HP NC552M Flex-10 (10GbaseKR)
- HP NC550SFP (SPF+/10GbaseSR)
- HP NC552SFP (SPF+/10GbaseSR)
- IBM System x 10GbE (SPF+/10GbaseSR)

# SEE ALSO

arp(4), ifmedia(4), intro(4), netintro(4), pci(4), hostname.if(5), ifconfig(8)

# HISTORY

The `oce` driver first appeared in OpenBSD 5.3.

# AUTHORS

The `oce` driver was written by Emulex and ported from FreeBSD by Mike Belopuhov.

January 28, 2018 | Debian