AXPPMIC(4) | Device Drivers Manual | AXPPMIC(4)

# NAME

`axppmic` — X-Powers AXP Power Management IC

# SYNOPSIS

`axppmic* at iic?`
`axppmic* at rsb?`

# DESCRIPTION

The `axppmic` driver provides support for the X-Powers AXP Power Management ICs. Depending on the model, these devices have temperature, voltage and current sensors and power indicators. Sensor values are made available through the sysctl(8) interface.

# SEE ALSO

iic(4), intro(4), sxirsb(4), sensorsd(8), sysctl(8)

# HISTORY

The `axppmic` device driver first appeared in OpenBSD 6.3.

# AUTHORS

The `axppmic` driver was written by Mark Kettenis <kettenis@openbsd.org>.

June 20, 2020 | Debian