GLENV(4) | Device Drivers Manual | GLENV(4)

# NAME

`glenv` — Genesys Logic GL518SM temperature, voltage, and fan sensor

# SYNOPSIS

`glenv* at iic?`

# DESCRIPTION

The `glenv` driver provides support for the Genesys Logic GL518SM hardware monitor to be used with the sysctl(8) interface.

The GL518SM possesses a voltage sensor, a temperature sensor and two fan speed sensors.

# SEE ALSO

iic(4), intro(4), sensorsd(8), sysctl(8)

# HISTORY

The `glenv` driver first appeared in OpenBSD 3.9.

# AUTHORS

The `glenv` driver was written by Mark Kettenis <kettenis@openbsd.org>.

July 16, 2013 | Debian