APLPINCTRL(4) | Device Drivers Manual (arm64) | APLPINCTRL(4)

# NAME

`aplpinctrl` — Apple pin multiplexing

# SYNOPSIS

`aplpinctrl* at fdt?`

# DESCRIPTION

The `aplpinctrl` driver uses pin control data from the device tree to select one of multiple possible roles available for pins on various Apple SoCs.

# SEE ALSO

intro(4)

# HISTORY

The `aplpinctrl` driver first appeared in OpenBSD 7.0.

# AUTHORS

The `aplpinctrl` driver was written by Mark Kettenis <kettenis@openbsd.org>.

August 31, 2021 | Debian