MVPINCTRL(4) | Device Drivers Manual | MVPINCTRL(4)

# NAME

`mvpinctrl` — Marvell Armada pin multiplexing

# SYNOPSIS

`mvpinctrl* at fdt?`

# DESCRIPTION

The `mvpinctrl` driver uses pin control data from the device tree to configure the MPP pins on Marvell Armada SoCs.

# SEE ALSO

intro(4)

# HISTORY

The `mvpinctrl` device driver first appeared in OpenBSD 6.3.

# AUTHORS

The `mvpinctrl` driver was written by Patrick Wildt <patrick@blueri.se> and Mark Kettenis <kettenis@openbsd.org>.

May 11, 2019 | Debian