UTRH(4) | Device Drivers Manual | UTRH(4)

# NAME

`utrh` — USBRH temperature and humidity sensor

# SYNOPSIS

`utrh* at uhidev?`

# DESCRIPTION

The `utrh` driver provides support for Strawberry Linux's USBRH device. The sensor possesses a collection of sensor values which are made available through the sysctl(8) interface. The humidity data unit is "%RH" and the temperature data unit is "degC".

# SEE ALSO

intro(4), uhidev(4), sensorsd(8), sysctl(8)

# AUTHORS

The `utrh` driver was written by Yojiro UO <yuo@nui.org>.

July 16, 2013 | Debian