BWTWO(4) | Device Drivers Manual (sparc64) | BWTWO(4)

# NAME

`bwtwo` — monochromatic frame buffer

# SYNOPSIS

`bwtwo* at sbus?`
`wsdisplay* at bwtwo?`

# DESCRIPTION

The `bwtwo` is an SBus monochrome frame buffer.

The `bwtwo` driver interfaces the frame buffer with the wscons(4) console framework. It does not provide direct device driver entry points but makes its functions available via the internal wsdisplay(4) interface.

# SEE ALSO

intro(4), sbus(4), wscons(4), wsdisplay(4)

March 31, 2008 | Debian