OCTUCTL(4) | Device Drivers Manual (octeon) | OCTUCTL(4)

# NAME

`octuctl` — OCTEON II USB controller interface

# SYNOPSIS

`octuctl0 at iobus? irq 56`
`ehci0 at octuctl?`
`ohci0 at octuctl?`

# DESCRIPTION

The `octuctl` driver provides support for the OCTEON II USB controller interface, which provides an interface to ehci(4) and ohci(4) devices.

# SEE ALSO

ehci(4), ohci(4)

# HISTORY

The `octuctl` driver first appeared in OpenBSD 6.0.

# AUTHORS

The `octuctl` driver was written by Jonathan Matthew <jmatthew@openbsd.org>.

September 18, 2016 | Debian