RTSX(4) | Device Drivers Manual | RTSX(4)

# NAME

`rtsx` — Realtek SD card reader

# SYNOPSIS

`rtsx* at pci?`
`sdmmc* at rtsx?`

# DESCRIPTION

The `rtsx` driver provides support for the Realtek RTS5209, RTS5227, RTS5229, RTS522A, RTS5249, RTS525A, RTL8402, RTL8411, and RTL8411B SD card readers.

The sdmmc(4) subsystem performs SD/MMC transactions to communicate with SD or SDHC devices inserted into the SD slot.

# SEE ALSO

intro(4), sdmmc(4)

# HISTORY

The `rtsx` driver first appeared in OpenBSD 5.3.

# AUTHORS

The `rtsx` driver was written by Stefan Sperling <stsp@openbsd.org>.

# BUGS

The `rtsx` driver does not support MS (Memory Stick) and xD (Extreme Digital) devices even though the hardware supports them.

Support for SDIO interrupts is not implemented.

September 6, 2017 | Debian