RGE(4) | Device Drivers Manual | RGE(4)

# NAME

`rge` — Realtek 8125/8126/8127 PCI Express 10/100/1Gb/2.5Gb/5Gb/10Gb Ethernet device

# SYNOPSIS

`rge* at pci?`

# DESCRIPTION

The `rge` driver provides support for NICs based on the Realtek RTL8125, RTL8126 and RTL8127 PCI Express Ethernet controllers, including the following:

- IOCrest IO-PCE8126-GLAN Adapter (5000baseT)
- Realtek 8125/8125B 2.5GbE Adapter (2500baseT)
- Rivet Networks Killer E3000 Adapter (2500baseT)
- TP-LINK TL-NG421 Adapter (2500baseT)

NICs based on the RTL8125 are capable of 10, 100, 1000 and 2500Mbps operation. NICs based on the RTL8126 are capable of 10, 100, 1000, 2500 and 5000Mbps operation. The RTL8127 supports 10Gbps speed.

The `rge` driver additionally supports Wake on LAN (WoL). See arp(8) and ifconfig(8) for more details.

# SEE ALSO

arp(4), ifmedia(4), intro(4), netintro(4), pci(4), hostname.if(5), ifconfig(8)

# HISTORY

The `rge` driver first appeared in OpenBSD 6.6.

# AUTHORS

The `rge` driver was written by Kevin Lo <kevlo@openbsd.org>.

September 19, 2025 | Debian