TLPHY(4) | Device Drivers Manual | TLPHY(4)

# NAME

`tlphy` — Texas Instruments ThunderLAN internal Ethernet PHY

# SYNOPSIS

`tlphy* at mii?`

# DESCRIPTION

The `tlphy` driver supports the internal PHY on TI ThunderLAN Ethernet interfaces. The ThunderLAN PHY supports 10base5 (AUI) and 10base2 (BNC) on some ThunderLAN implementations.

# SEE ALSO

ifmedia(4), intro(4), mii(4), ifconfig(8)

July 31, 2009 | Debian