APIO(4) | Device Drivers Manual (sparc64) | APIO(4)

# NAME

`apio` — SBus Aurora pio1 driver

# SYNOPSIS

`apio* at sbus?`
`lpt* at apio?`

# DESCRIPTION

The `apio` driver provides support for the Aurora Technologies pio1 parallel port interface, which is basically an lpt(4) port with sbus(4) glue logic.

# SEE ALSO

intro(4), lpt(4), sbus(4)

# HISTORY

OpenBSD support for `apio` was added in OpenBSD 3.1.

# AUTHORS

The driver was written by Jason Wright <jason@thought.net>.

# BUGS

Only revision 210sj is known to work. Minor work may be necessary for other revisions of this card.

July 16, 2013 | Debian