UAQ(4) | Device Drivers Manual | UAQ(4)

# NAME

`uaq` — Aquantia AQC111U/AQC112U 100/1Gb/2.5Gb/5Gb USB Ethernet device

# SYNOPSIS

`uaq* at uhub?`

# DESCRIPTION

The `uaq` driver provides support for USB Ethernet adapters based on the Aquantia AQC111U and AQC112U chipsets, including the following:

Aquantia AQtion USB to 5GbE Controller
ASIX USB 3.1 Gen1 to 5G Multi-Gigabit Ethernet Adapter
ASIX USB 3.1 Gen1 to 2.5G Multi-Gigabit Ethernet Adapter
QNAP QNA-UC5G1T USB to 5GbE Adapter
Sabrent NT-SS5G USB to 5GbE Adapter
StarTech USG5GA30 USB to 5GbE Adapter
TRENDnet TUC-ET5G USB-C 3.1 to 5GBASE-T Ethernet Adapter

The AQC111U and AQC112U contain an integrated Multi-Gig Ethernet MAC and PHY, supporting 100, 1000, 2500 and, in the AQC111U, 5000Mbps operation.

For more information on configuring this device, see ifconfig(8).

# SEE ALSO

arp(4), ifmedia(4), mii(4), netintro(4), uhub(4), usb(4), hostname.if(5), ifconfig(8)

# HISTORY

The `uaq` device driver first appeared in OpenBSD 7.0.

# AUTHORS

The `uaq` driver was written by Jonathan Matthew <jmatthew@openbsd.org>.

May 15, 2022 | Debian