INTRO(4) | Device Drivers Manual (hppa) | INTRO(4)

# NAME

`intro` — introduction to special files and hardware support

# DESCRIPTION

This section describes the special files, related driver functions, and networking support available in the system. In this part of the manual, the SYNOPSIS section of each configurable device gives a sample specification for use in constructing a system description for the config(8) program. The DIAGNOSTICS section lists messages which may appear on the console and/or in the system error log /var/log/messages due to errors in device operation; see syslogd(8) for more information.

This section contains both devices which may be configured into the system and network related information. The networking support is introduced in netintro(4).

# DEVICE SUPPORT

This section describes the hardware supported on the HP PA-RISC platform. Software support for these devices comes in two forms. A hardware device may be supported with a character or block device driver, or it may be used within the networking subsystem and have a network interface driver. Character and block devices are accessed through files in the file system of a special type; see mknod(8). Network interfaces are indirectly accessed through the interprocess communication facilities provided by the system; see socket(2).

A hardware device is identified to the system at configuration time and the appropriate device or network interface driver is then compiled into the system. When the resultant system is booted, the autoconfiguration facilities in the system probe for the device and, if found, enable the software support for it. If a device does not respond at autoconfiguration time, it is not accessible at any time afterwards. To enable a device which did not autoconfigure, the system must be rebooted.

The autoconfiguration system is described in autoconf(4).

# SUPPORTED SYSTEMS

A list of HP 9000/700 models targeted for support is listed below, including basic system characteristics.

Model | MHz | CPU | Caches, KB | Expansion
705 | 35 | 7000 | 32/64 | N/A
710 | 50 | 7000 | 32/64 | N/A
720 | 50 | 7000 | 128/256 | EISA, GSC
730 | 66 | 7000 | 128/256 | EISA, GSC
750 | 66 | 7000 | 256/256 | 4 EISA, 2 SGC
715 | 33 | 7100 | 64/64 | EISA/SGC
715 | 50 | 7100 | 64/64 | EISA/SGC
715 | 75 | 7100 | 256/256 | EISA/SGC
725 | 50 | 7100 | 64/64 | 3 EISA, EISA/SGC
725 | 75 | 7100 | 256/256 | 3 EISA, EISA/SGC
735 | 100 | 7100 | 256/256 | EISA, SGC
742i | 50 | 7100 | 64/64 | N/A
745i | 50 | 7100 | 64/64 | 4 EISA
745i | 100 | 7100 | 256/256 | 4 EISA
747i | 50 | 7100 | 64/64 | 2 EISA, SGC, 6 VME
747i | 100 | 7100 | 256/256 | 2 EISA, SGC, 6 VME
755 | 100 | 7100 | 256/256 | 4 EISA, 2 SGC
735 | 125 | 7150 | 256/256 | EISA, SGC
755 | 125 | 7150 | 256/256 | 4 EISA, 2 SGC
712 | 60 | 7100LC | 32/32 | GIO, TSIO
712 | 80 | 7100LC | 128/128 | GIO, TSIO
712 | 100 | 7100LC | 128/128 | GIO, TSIO
715 | 64 | 7100LC | 128/128 | EISA/GSC
715 | 80 | 7100LC | 128/128 | EISA/GSC
715 | 100 | 7100LC | 128/128 | EISA/GSC
715XC | 100 | 7100LC | 512/512 | EISA/GSC
725 | 64 | 7100LC | 128/128 | EISA, 3 EISA/GSC
725 | 100 | 7100LC | 128/128 | EISA, 3 EISA/GSC
743i | 64 | 7100LC | 128/128 | 2 GSC-M/2(4), VME
743i | 100 | 7100LC | 128/128 | 2 GSC-M/2(4), VME
748i | 64 | 7100LC | 128/128 | 2 GSC-M/2(4), 4 EISA/PCI, 6 VME
748i | 100 | 7100LC | 128/128 | 2 GSC-M/2(4), 4 EISA/PCI, 6 VME
SAIC | 60 | 7100LC | 32/32 | GIO, TSIO, 2 PCMCIA
SAIC | 80 | 7100LC | 128/128 | GIO, TSIO, 2 PCMCIA
J200 | 100 | 7200 | 256/256 | GSC, 2 EISA, 2 EISA/GSC
J210 | 120 | 7200 | 256/256 | GSC, 2 EISA, 2 EISA/GSC
J210XC | 120 | 7200 | 1MB/1MB | GSC, 2 EISA, 2 EISA/GSC
C100 | 100 | 7200 | 256/256 | GSC, 3 EISA/GSC
C110 | 120 | 7200 | 256/256 | GSC, 3 EISA/GSC
744 | 132 | 7300LC | 64/64 | 2 GSC-M/2(4), VME
744 | 165 | 7300LC | 64/64+512 | 2 GSC-M/2(4), VME
745 | 132 | 7300LC | 64/64 | 2 GSC-M/2(4), 4 EISA/PCI
745 | 165 | 7300LC | 64/64+512 | 2 GSC-M/2(4), 4 EISA/PCI
748 | 132 | 7300LC | 64/64 | 2 GSC-M/2(4), 4 EISA/PCI, 6 VME
748 | 165 | 7300LC | 64/64+512 | 2 GSC-M/2(4), 4 EISA/PCI, 6 VME
A180 | 180 | 7300LC | 64/64 | 2 HSC/PCI
A180C | 180 | 7300LC | 64/64+1MB | 2 HSC/PCI
B132L | 132 | 7300LC | 64/64(+1MB) | GSC/PCI, GSC/PCI/EISA
B132L+ | 132 | 7300LC | 64/64(+1MB) | GSC/PCI, GSC/PCI/EISA
B160L | 160 | 7300LC | 64/64(+1MB) | GSC/PCI, GSC/PCI/EISA
B180L+ | 180 | 7300LC | 64/64(+1MB) | GSC/PCI, GSC/PCI/EISA
C132L | 132 | 7300LC | 64/64(+1MB) | 2 GSC/PCI/EISA, 2 GSC/EISA
C160L | 160 | 7300LC | 64/64(+1MB) | 2 GSC/PCI/EISA, 2 GSC/EISA
RDI | 132 | 7300LC | 64/64(+1MB) | 2 CardBus
RDI | 160 | 7300LC | 64/64(+1MB) | 2 CardBus
RDI | 180 | 7300LC | 64/64(+1MB) | 2 CardBus
C160 | 160 | 8000 | 512/512 | 2 GSC/PCI/EISA, 2 GSC/EISA
C180 | 180 | 8000 | 1024/1024 | 2 GSC/PCI/EISA, 2 GSC/EISA
J280 | 180 | 8000 | 1024/1024 | 3 GSC/PCI, PCI, PCI/EISA
J282 | 180 | 8000 | 1024/1024 | 3 GSC/PCI, PCI, PCI/EISA
C200 | 200 | 8200 | 512/1024 | GSC/PCI/EISA, 3 GSC/PCI
C240 | 240 | 8200 | 2048/2048 | GSC/PCI/EISA, 3 GSC/PCI
J2240 | 240 | 8200 | 2048/2048 | 3 GSC/PCI, PCI, PCI/EISA
B1000 | 300 | 8500 | 512/1024 | 6 PCI
C360 | 360 | 8500 | 512/1024 | GSC/PCI/EISA, 3 GSC/PCI
B2000 | 400 | 8500 | 512/1024 | 4 PCI
C3000 | 400 | 8500 | 512/1024 | 6 PCI
J5000 | 440 | 8500 | 512/1024 | 7 PCI
J7000 | 440 | 8500 | 512/1024 | 7 PCI
B2600 | 500 | 8600 | 512/1024 | 4 PCI
C3600 | 552 | 8600 | 512/1024 | 6 PCI
J5600 | 552 | 8600 | 512/1024 | 7 PCI
J6000 | 552 | 8600 | 512/1024 | 7 PCI
J7600 | 552 | 8600 | 512/1024 | 7 PCI
C3650 | 625 | 8700 | 768/1536 | 6 PCI
C3700 | 750 | 8700 | 768/1536 | 6 PCI
J6700 | 750 | 8700 | 768/1536 | 3 PCI
C3750 | 875 | 8700+ | 768/1536 | 6 PCI
J6750 | 875 | 8700+ | 768/1536 | 3 PCI

# LIST OF DEVICES

A complete list of available devices is contained within the pages describing the system buses and controllers. For example, a PCI device would be listed in the pci(4) man page. The following buses and controllers list these devices:

cardbus(4)
  introduction to CardBus support
gsc(4)
  introduction to HP 9000/700 GSC bus support
hil(4)
  introduction to HP-HIL support
onewire(4)
  1-Wire bus
pci(4)
  introduction to PCI bus support
pcmcia(4)
  introduction to PCMCIA (PC Card) support
usb(4)
  introduction to Universal Serial Bus support

# SEE ALSO

autoconf(4), cpu(4), io(4), runway(4), config(8)

# HISTORY

The hppa `intro` first appeared with OpenBSD 3.1.

March 31, 2022 | Debian