OWSBM(4) | Device Drivers Manual | OWSBM(4)

# NAME

`owsbm` — 1-Wire smart battery monitor device

# SYNOPSIS

`owsbm* at onewire?`

# DESCRIPTION

The `owsbm` driver provides support for the 1-Wire smart battery monitor. The sensor possesses a temperature sensor, an A/D converter for measuring both battery voltage and current, a current accumulator of both incoming and outgoing current, an elapsed time and 40 bytes of nonvolatile EEPROM.

Only the three voltages (VDD, VAD, CR) and temperature are accessible by the sysctl(8) interface.

The following chips are supported by the driver:

- Maxim/Dallas DS2438

# MEASURING CURRENT

The sensor does not measure current directly. Instead it measures the voltage across the Rsens pins.

    I = Voltage CR / Rsens    (where Rsens is in Ohms)

# SEE ALSO

intro(4), onewire(4), owtemp(4), sysctl(8)

# HISTORY

The `owsbm` driver first appeared in OpenBSD 4.1.

# AUTHORS

The `owsbm` driver was written by Aaron Linville <aaron@linville.org>.

July 16, 2013 | Debian