UGEN(4) | Device Drivers Manual | UGEN(4)

# NAME

`ugen` — USB generic device support

# SYNOPSIS

`ugen* at uhub?`

# DESCRIPTION

The `ugen` driver provides support for all USB devices that do not have a special driver. It supports access to all parts of the device, but not in a way that is as convenient as a special purpose driver.

There can be up to 127 USB devices connected to a USB bus. Each USB device can have up to 16 endpoints. Each of these endpoints will communicate in one of four different modes: control, isochronous, bulk, or interrupt. Each of the endpoints will have a different device node. The four least significant bits in the minor device number determine which endpoint the device accesses and the rest of the bits determine which USB device.

If an endpoint address is used both for input and output, the device can be opened for both read or write.

To find out what endpoints exist there are a series of ioctl(2) operations available for the control endpoint that return the USB descriptors of the device, configurations, interfaces, and endpoints.

The control transfer mode can only happen on the control endpoint, which is always endpoint 0. Control requests are issued by ioctl(2) calls.

The bulk transfer mode can be in or out depending on the endpoint. To perform I/O on a bulk endpoint read(2) and write(2) should be used. All I/O operations on a bulk endpoint are unbuffered.

The interrupt transfer mode can only be in. To perform input from an interrupt endpoint read(2) should be used. A moderate amount of buffering is done by the driver.

All endpoints handle the following ioctl(2) calls:

`USB_SET_SHORT_XFER (int)`
  Allow short read transfer. Normally a transfer from the device which is shorter than the request specified is reported as an error.

`USB_SET_TIMEOUT (int)`
  Set the timeout on the device operations, the time is specified in milliseconds. The value 0 is used to indicate that there is no timeout.

The control endpoint (endpoint 0) handles the following ioctl(2) calls:

`USB_GET_CONFIG (int)`
  Get the device configuration number.

`USB_SET_CONFIG (int)`
  Set the device into the given configuration number. This operation can only be performed when the control endpoint is the sole open endpoint.

`USB_GET_ALTINTERFACE (struct usb_alt_interface)`
  Get the alternative setting number for the interface with the given index. The uai_config_index is ignored in this call.

      struct usb_alt_interface {
      	int	uai_config_index;
      	int	uai_interface_index;
      	int	uai_alt_no;
      };

`USB_SET_ALTINTERFACE (struct usb_alt_interface)`
  Set the alternative setting to the given number in the interface with the given index. The uai_config_index is ignored in this call.

  This operation can only be performed when no endpoints for the interface are open.

`USB_GET_NO_ALT (struct usb_alt_interface)`
  Return the number of different alternate settings in the uai_alt_no field.

`USB_GET_DEVICE_DESC (usb_device_descriptor_t)`
  Return the device descriptor.

`USB_GET_CONFIG_DESC (struct usb_config_desc)`
  Return the descriptor for the configuration with the given index. For convenience the current configuration can be specified by `USB_CURRENT_CONFIG_INDEX`.

      struct usb_config_desc {
      	int	ucd_config_index;
      	usb_config_descriptor_t ucd_desc;
      };

`USB_GET_INTERFACE_DESC (struct usb_interface_desc)`
  Return the interface descriptor for an interface specified by its configuration index, interface index, and alternative index. For convenience the current alternative can be specified by `USB_CURRENT_ALT_INDEX`.

      struct usb_interface_desc {
      	int	uid_config_index;
      	int	uid_interface_index;
      	int	uid_alt_index;
      	usb_interface_descriptor_t uid_desc;
      };

`USB_GET_ENDPOINT_DESC (struct usb_endpoint_desc)`
  Return the endpoint descriptor for the endpoint specified by its configuration index, interface index, alternative index, and endpoint index.

      struct usb_endpoint_desc {
      	int	ued_config_index;
      	int	ued_interface_index;
      	int	ued_alt_index;
      	int	ued_endpoint_index;
      	usb_endpoint_descriptor_t ued_desc;
      };

`USB_GET_FULL_DESC (struct usb_full_desc)`
  Return all the descriptors for the given configuration.

      struct usb_full_desc {
      	int	ufd_config_index;
      	u_int	ufd_size;
      	u_char	*ufd_data;
      };

  The ufd_data field should point to a memory area of the size given in the ufd_size field. The proper size can be determined by first issuing a `USB_GET_CONFIG_DESC` and inspecting the wTotalLength field.

`USB_DO_REQUEST`
  Send a USB request to the device on the control endpoint. Any data sent to/from the device is located at ucr_data. The size of the transferred data is determined from the ucr_request. The ucr_addr field is ignored in this call.

      struct usb_ctl_request {
      	int	ucr_addr;
      	usb_device_request_t ucr_request;
      	void	*ucr_data;
      	int	ucr_flags;
      #define	USBD_SHORT_XFER_OK	0x04	/* allow short reads */
      	int	ucr_actlen;	/* actual length transferred */
      };

  This is a dangerous operation in that it can perform arbitrary operations on the device. Some of the most dangerous (e.g., changing the device address) are not allowed.

`USB_GET_DEVICEINFO (struct usb_device_info)`
  Get an information summary for the device. This call will not issue any USB transactions.

Note that there are two different ways of addressing configurations, interfaces, alternatives, and endpoints: by index or by number. The index is the ordinal number (starting from 0) of the descriptor as presented by the device. The number is the respective number of the entity as found in its descriptor. Enumeration of descriptors use the index, getting and setting typically uses numbers.

Example: All endpoints (except the control endpoint) for the current configuration can be found by iterating the interface_index from 0 to config_desc->bNumInterfaces-1 and for each of these iterating the endpoint_index from 0 to interface_desc->bNumEndpoints-1. The config_index should be set to `USB_CURRENT_CONFIG_INDEX` and alt_index should be set to `USB_CURRENT_ALT_INDEX`.

# FILES

/dev/ugenN.EE
  Endpoint EE of device N.

# SEE ALSO

intro(4), uhub(4), usb(4)

# HISTORY

The `ugen` driver appeared in OpenBSD 2.6.

# BUGS

The driver is not yet finished; there is no access to isochronous endpoints.

March 31, 2022 | Debian