PAS(4) | Device Drivers Manual (i386) | PAS(4)

# NAME

`pas` — Media Vision Pro AudioSpectrum audio device

# SYNOPSIS

`pas0 at isa? port 0x220 irq 7 drq 1`
`audio* at pas?`

# DESCRIPTION

The `pas` driver provides support for second generation Media Vision Pro AudioSpectrum sound cards. These cards contain an MVD101 multimedia chip.

The following cards are supported:

    CDPC
    Fusion CD
    Fusion CD 16
    PAS 16
    PAS Plus

# SEE ALSO

audio(4), intro(4), isa(4)

May 31, 2007 | Debian