SMFB(4) | Device Drivers Manual (loongson) | SMFB(4)

# NAME

`smfb` — Silicon Motion frame buffer

# SYNOPSIS

`smfb* at pci?` (SM712)
`smfb* at voyager?` (SM502)

# DESCRIPTION

The `smfb` driver supports Silicon Motion SM502 and SM712 frame buffers in 16-bit color mode.

The `smfb` driver interfaces the frame buffer with the wscons(4) console framework, as a wsdisplay(4) device.

It is currently not possible to change the frame buffer resolution and color depth.

# SEE ALSO

intro(4), pci(4), voyager(4), wscons(4), wsdisplay(4)

February 18, 2010 | Debian