BCMSTBINTC(4) | Device Drivers Manual | BCMSTBINTC(4)

# NAME

`bcmstbintc` — Broadcom Set-to Box interrupt controller

# SYNOPSIS

`bcmstbintc* at fdt?`

# DESCRIPTION

The `bcmstbintc` driver provides support for the L2 interrupt controller integrated on Broadcom Set-top Box SoCs. This includes the Broadcom BCM2712 SoC that is used in the Raspberry Pi 5.

# SEE ALSO

intro(4)

# HISTORY

The `bcmstbintc` driver first appeared in OpenBSD 7.8.

# AUTHORS

The `bcmstbintc` driver was written by Mark Kettenis <kettenis@openbsd.org>.

September 8, 2025 | Debian