PHANTOMAS(4) | Device Drivers Manual (hppa) | PHANTOMAS(4)

# NAME

`phantomas` — Phantom PseudoBC GSC+ Port

# SYNOPSIS

`phantomas0 at mainbus?`
`dino* at phantomas?`
`lasi* at phantomas?`
`sti* at phantomas?`
`wax* at phantomas?`

# DESCRIPTION

The Phantom bus converter is used to connect various devices and controllers to the system bus, where the processor and memory are located. Currently the following are connected: the sti(4) graphics interface; the lasi(4) and wax(4) bus host adapters for gsc(4); and the dino(4) PCI bridge.

# SEE ALSO

dino(4), gsc(4), intro(4), lasi(4), sti(4), wax(4)

# HISTORY

The `phantomas` driver appeared in OpenBSD 3.3.

December 22, 2020 | Debian