UGOLD(4) | Device Drivers Manual | UGOLD(4)

# NAME

`ugold` — TEMPer gold HID thermometer and hygrometer

# SYNOPSIS

`ugold* at uhidev?`

# DESCRIPTION

The `ugold` driver provides support for PCsensors TEMPer gold devices. The following devices are supported by the `ugold` driver:

Device | Sensors
`RDing TEMPer1V1.2` | 1 Temperature
`RDing TEMPerV1.4` | 1 Temperature
`RDing TEMPer1F_V4.1` | 1 Temperature (external)
`RDing TEMPer2_V4.1` | 2 Temperature (internal/external)
`RDing TEMPerGold_V3.1` | 1 Temperature
`RDing TEMPerGold_V3.4` | 1 Temperature
`RDing TEMPerGold_V3.5` | 1 Temperature
`RDing TEMPerHum1V1.0` | 1 Temperature and 1 Humidity
`RDing TEMPerHum1V1.2` | 1 Temperature and 1 Humidity
`RDing TEMPerHUM_V3.9` | 1 Temperature and 1 Humidity
`RDing TEMPerHUM_V4.0` | 1 Temperature and 1 Humidity
`RDing TEMPerHUM_V4.1` | 1 Temperature and 1 Humidity
`RDing TEMPer1F_H1V1.5F` | 1 Temperature and 1 Humidity
`RDing TEMPerX_V3.1` | 1 Temperature and 1 Humidity
`RDing TEMPerX_V3.3` | 1 Temperature and 1 Humidity

The driver possesses a collection of sensor values which are made available through the sysctl(8) interface.

# SEE ALSO

intro(4), uhidev(4), sensorsd(8), sysctl(8)

# HISTORY

The `ugold` driver first appeared in OpenBSD 5.5.

# AUTHORS

The `ugold` driver was written by Takayoshi SASANO <uaa@openbsd.org> and Martin Pieuchot <mpi@openbsd.org>.

TEMPerHUM support was added by Joerg Jung <jung@openbsd.org>.

# CAVEATS

Linearization and temperature compensation for the humidity values of the TEMPerHUM1V1.0 is not implemented.

July 27, 2024 | Debian